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ANNEXURE-[[H03]]
Test Report No.: ECT/16018/BC/ [[TCNo]] 						Date: [[TCDate2]]

Resistance to Corrosion (External) test as per Clause 6.6

Sample Quantity: One sample from the same family

Test method:

· Subject fully charged extinguishers, to a salt spray test for a period of 120 hrs.
· Drying period of at least 24 h at room temperature
· Carefully wash the extinguisher to remove any salt deposits

	 [[ProductDesc]] 

	Sr. Nos.
	Capacity
	Cylinder Sr. Nos.
	      Date

	1
	[[Cap1]]
	[[SrNo1_4]]
	[[TCDate2]]

	2
	[[Cap2]]
	[[SrNo2_4]]
	[[TCDate2]]

	3
	[[Cap3]]
	[bookmark: _GoBack][[SrNo3_4]]
	[[TCDate2]]




Observations:

	Type of check
	Requirement 
	Result 

	Mechanical operation of all working parts
	Shall be unimpaired
	Found satisfactorily

	The pressure gauge (if fitted)
	Shall remain functional and water tight
	No Pressure Gauge provided

	Corrosion of the metal
	a) Shall be no corrosion of the metal of extinguisher body
b) Discoloration/superficial corrosion of non-ferrous metal is acceptable
c) Galvanic corrosion between dissimilar metals shall not  be permitted
	Found satisfactorily

	Minimum effective discharge time and method of operation
	Shall comply specified requirements
	Found satisfactorily
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