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                                                                                                          ANNEXURE-[[H06]]
Test Report No.: FTB/16018/BC/ [[TCNo]] 						Date: [[TCDate2]]

Class B rating suitability test as per Clause 7.3 

    
Test Requirements as per IS 16018:2012 Clause 7.3
Operator’s clothing- Shoes, helmet, visor, gloves, etc. 

Observations:


	[[ProductDesc]] 

	Sr.No.
	Capacity 
	Cylinder Sr. Nos.
	Fire Rating

	
	
	
	

	
	
	
	

	1
	[[Cap1]]
	[[SrNo1_8]]
	20B

	2
	[[Cap2]]
	[[SrNo2_8]]
	20B

	3
	[[Cap3]]
	[bookmark: _GoBack][[SrNo3_8]]
	 







	Sr. No.
	Particulars 
	Requirements 
	Remarks 

	01
	Addition of liquid (Volume of liquid)
	Max. liquid depth 50mm
Min. Heptane depth 15mm
	Found Satisfactorily

	
	Extinguishment
	All flames shall be extinguished
	Found Satisfactorily

	02
	Addition of liquid (Volume of liquid)
	Max. liquid depth 50mm
Min. Heptane depth 15mm
	Found Satisfactorily

	
	Extinguishment
	All flames shall be extinguished
	Found Satisfactorily
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