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 										ANNEXURE-[[H08]]
Test Report No.: PMST/16018/ BC/ [[TCNo]]  					Date: [[TCDate3]]

Pressure Cycling Test as per Clause 8.3.3


Test Procedure:
One cylinder of each size and type shall sustain without rupture 100 cycles from 0 to test pressure (Pt) and back to 0 at the rate of 3 cycles per min. 
Requirement:
At the conclusion of testing the cylinder shall be subjected to and comply with burst test.

Observations:

	 

	Sr. No.
	Capacity 
	Cylinder Sr. Nos.
	Date of Test
	Remarks

	1
	[[Cap1]]
	[[SrNo1_12]]
	[[TCDate3]]
	No burst observed found ok

	2
	[[Cap2]]
	[[SrNo2_12]]
	[[TCDate3]]
	No burst observed found ok

	3
	[[Cap3]]
	[bookmark: _GoBack][[SrNo3_12]]
	[[TCDate3]]
	No burst observed found ok
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