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Test Report No.: INT/ [[TCNo]]		           						Date: [[TCDate2]]
ANNEXURE-[[M06]]
Intermittent Discharge test Clause 7.8

Test Method:

Operate the extinguisher intermittently by opening and closing the valve in cycles of 2s open 2 s closed until the end of discharge is reached.

Note: For cartridge operated extinguishers, pierce the cartridge and allow the pressure to build for 6 s before opening the control valve.

Test requirement:

 At the end of discharge test, the extinguishers shall not retain,
a. Powder : 15 percent
b. All other : 10 percent

Test procedure:

Condition the fully charged extinguishers at 27±5⁰C and 60±5⁰C, each at minimum 18 hr.
	[[ProductDesc]]
	[[Cap1]]
	[[Cap2]]
	[[Cap3]]
	[[Cap4]]
	[[Cap5]]

	Cylinder Sr. Nos.
	[[SrNo1_7]]
	[[SrNo2_7]]
	[[SrNo3_7]]
	[[SrNo4_7]]
	[[SrNo5_7]]





	Store Temperature
	Duration
	Start Time
	End Time

	27 ± 5°C
	18 h
	10:30  AM
	04:30 PM

	60 ± 5°C
	18 h
	04:30  PM
	10:30 AM



Observations:

	Cylinders 
Sr. No.
	Retain percentage
	Remarks

	
	Requirement
	Observation
	

	[[SrNo1_7]]
	Powder: Not more than 15% 
All other: Not more than 10%
	[[R]:R5-6] %
	Pass

	                [[SrNo2_7]]
	
	[[R]:R5-6] %
	Pass

	[[SrNo3_7]]
	
	[[R]:R5-6] %
	Pass

	                [[SrNo4_7]]
	
	               [[R]:R4-6] %
	Pass

	                 [[SrNo5_7]]
	
	[bookmark: _GoBack]                [[R]:R5-6] %
	Pass
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