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[bookmark: _GoBack]ANNEXURE-[[M07]]

Determination of Maximum Service Pressure (PMS) Clause 9.2.1.8

      
Test Method:
     
Condition the extinguisher for 18 h at a temperature 60±5 °C. 
For stored pressure extinguishers determine the pressure immediately after taking each extinguisher out of the oven. 
For cartridge operated extinguishers activate the cartridge immediately

Requirement:

For each type of extinguishers the highest pressure observed during test is recorded as the maximum service pressure.

Observations:

	[[ProductDesc]]
	Cylinder 
Sr. Nos.
	Start and end time of conditioning
	Observed PMS (in bar)

	[[Cap1]]
	[[SrNo1_8]]
	4:15 PM
To
10:15 AM
	[[R]:R17-20]

	[[Cap2]]
	[[SrNo2_8]]
	
	[[R]:R17-20]

	[[Cap3]]
	[[SrNo3_8]]
	
	[[R]:R17-20]

	[[Cap4]]
	[[SrNo4_8]]
	
	[[R]:R17-20]

	[[Cap5]]
	[[SrNo5_8]]
	
	[[R]:R17-20]
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