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[bookmark: _GoBack]ANNEXURE-[[M09]]
Pressure cycling test as per Clause 9.2.4

Test method:

One cylinder shall be tested. 
Extinguisher shall sustain without rupture 5000 cycles from 0 to test pressure (Pt) and back to 0 at the rate of 6 cycles per min. 
 
Test requirements:

At the conclusion of testing the cylinder shall be subjected to and comply with burst test. 

Observations:

	[[ProductDesc]]
	[[Cap1]]
	[[Cap2]]
	[[Cap3]]
	[[Cap4]]
	[[Cap5]]

	Cylinder Sr. Nos.
	[[SrNo1_10]]
	[[SrNo2_10]]
	[[SrNo3_10]]
	[[SrNo4_10]]
	[[SrNo5_10]]

	Shall comply to burst test requirements

	Observation
	Pass
	Pass
	Pass
	Pass
	Pass



[image: MUKESHBHAI]     [image: ]                                                                                            
QC Assistant		                                                            QC In charge
image1.jpeg
@Qd‘[ @d





image2.png




