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Test Report No.: [[TCNo]]		           						Date: [[TCDate3]]

ANNEXURE-[[M12]]   
Class ‘A’ Test Fire Clause 8.3 
 

Test method, Procedure and requirements:

Operator’s clothing- Operator shall wear Shoes, helmet, visor and gloves.
Location: Cl. No. 8.3.1 of IS 15683:2018
Air Inlet Opening- provided as per table 5 Cl. 8.31 of IS 15683:2018
Construction of Wood crib- as per table 6 of Cl. No. 8.3.2 of IS 15683:2018
Ignition Pan Size and fuel quality- as per table 7 of Cl. No. 8.3.2 of IS 15683:2018

Requirements for extinguishment Cl. 8.2.2 (a):
All flames are extinguished. There shall be no flames visible 3 min. after complete discharge of the extinguisher. The appearance of non persistent flames during the 3 min period shall be ignored. Non persistent flames are defined as less than 50 mm in height and less than 1 min duration; if the crib collapses during the test, it shall be considered as void and fresh test carried out.
Observations:

	[[ProductDesc]]
	[[Cap1]] 
	[[Cap2]]
	[[Cap3]]
	[[Cap4]]
	[[Cap5]]

	Cylinder Sr. No.
	[[SrNo1_12]]
	[[SrNo2_12]]
	[[SrNo3_12]]
	[[SrNo4_12]]
	[bookmark: _GoBack][[SrNo5_12]]

	Fire Rating
	1A
	2A
	3A
	4A
	6A

	Observation 

	No flames visible 10min after complete discharge
	Pass
	Pass
	Pass
	Pass
	Pass

	Non-persistent flames shall be ignored
	Pass
	Pass
	Pass
	Pass
	Pass
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