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Test Report No.: FTB/ [[TCNo]]	           						Date: [[TCDate3]]

ANNEXURE-[[M13]]   
Class ‘B’ Test Fire Clause 8.4 
 

Test method, Procedure and requirements:

Operator’s clothing- Operator shall wear Shoes, helmet, visor and gloves. 
Location: Cl. No. 8.4.1 of IS 15683:2018
Construction - as per table 8 of Cl. No. 8.4.2 of IS 15683:2018
Fuel: Commercial grade n-heptane having an boiling point of not less than 88⁰C and final boiling point not more than 105.

Test Requirements: All flames are extinguished

Observations:

	[[ProductDesc]]
	[[Cap1]] 
	[[Cap2]]
	[[Cap3]]
	[[Cap4]]
	[[Cap5]]

	Cylinder Sr. No.
	[[SrNo1_13]]
	[[SrNo2_13]]
	[[SrNo3_13]]
	[[SrNo4_13]]
	[bookmark: _GoBack][[SrNo5_13]]

	Fire Rating
	21B
	34B
	89B
	144B
	183B

	Observation 

	Liquid depth 
(water + heptane)
	50 mm

	No flames visible 10min after complete discharge
	Pass

	Non-persistent flames shall be ignored
	All flames extinguished
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