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        										   ANNEXURE-[[M16]]

Electrical Conductivity of Extinguisher Discharge Clause 8.8

      

Test Method:
     
Connect a metal plate to a transformer so that alternating voltage of 36 ±3.6kV is established between the plate and the earth. Mount the extinguisher on an insulating support with the nozzle/handle fixed 1 m from the center of the plate.

Measure any current flowing between the earth and the extinguisher when the plate is live and the extinguisher discharging.

Requirement:

The current between the handle/nozzle and earth and between the earth and extinguisher shall be no more than 0.5 mA at any time during the complete discharge duration of the extinguisher.

Observations:

	[[ProductDesc]]

	Capacity
	Cylinder
	Observed Current (mA)
	Conclusion

	[[Cap1]]
	[[SrNo1_17]]
	[[R]:R0.2-0.3]
	PASS

	[[Cap2]]
	[[SrNo1_17]]
	[[R]:R0.2-0.3]
	PASS

	[[Cap3]]
	[[SrNo1_17]]
	[[R]:R0.3-0.4]
	PASS

	[[Cap4]]
	[[SrNo1_17]]
	[[R]:R0.3-0.4]
	PASS

	[[Cap5]]
	[[SrNo1_17]]
	[[R]:R0.3-0.4]
	PASS
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