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ANNEXURE-[[M14]]   
Class ‘F’ Test Fire Clause 8.6 
 

Test method, Procedure and requirements:

Operator’s clothing- Operator shall wear Shoes, helmet, visor and gloves.
Location: Cl. No. 8.6.1 of IS 15683:2018
Construction of apparatus- as per Fig. 3/4 of Cl. No. 8.6.2 of IS 15683:2018
Ignition tray Size and fuel quality- as per of Cl. No. 8.6.3 of IS 15683:2018

Requirements for extinguishment Cl. 8.2.2 (c):
All flames are extinguished. There shall be no re-ignition of the vegetable oil for 3 minutes after discharge.                                                                                                                                                                                                                                                           
Observations:

	[[ProductDesc]]
	[[Cap1]] 
	[[Cap2]]
	[[Cap3]]
	[[Cap4]]
	[[Cap5]]

	Cylinder Sr. No.
	[[SrNo1_14]]
	[[SrNo2_14]]
	[[SrNo3_14]]
	[[SrNo4_14]]
	[[SrNo5_14]]

	Fire Rating
	5F
	5F
	15F
	25F
	75F

	Observation 

	No flames visible 3 min after complete discharge
	No flames visible

	No re-ignition of vegetable oil for 3 minutes after discharge.
	No re-ignition
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